{"text_format":"2","workbook":"xlsx","n_sheets":6,"sheets":["整车功耗测试","液压测试","北醒测试","放大晶体管测试","光电测试","整车功耗测试原始资料图"],"not_rendered":{"charts":0,"images":9,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"整车功耗测试","index":0,"n_rows":38,"n_cols":7,"rows_kept":38,"cut":false,"hidden":false,"merged":[]}
[]
[null,"测试目的：","了解整车各个环节的瞬时功率，确定电池与电源模块的选型合理性。完善设计文档。估算运行时长与充电时长"]
[]
[null,"测试说明：","测量各个分支的电流与电压，确定额定功率与最大功率值"]
[]
[]
[]
[null,"电气图"]
{"$rows_empty":19}
[null,"电池测试数据"]
[]
[null,"状态","电压（mV）","电流(mA)","功耗（W）","容量（%）","温度（℃）"]
[null,"停止空载",52970,770,40.786900000000003,87,6]
[null,"转速1500，空载",52970,3440,182.21680000000001,87,6]
[null,"转速3000，空载",52970,5880,311.05200000000002,87,6]
[null,"停止满载",52970,770,40.786900000000003,87,6]
[null,"转速1500，满载",52970,4080,215.83199999999999,87,6]
[null,"转速3000，满载",52970,17050,903.13850000000002,87,6]
[null,"换向满载",52970,21510,1139.3847000000001,87,6]
[null,"顶升满载",52970,21460,1136.7362000000001,87,6]

{"sheet":"液压测试","index":1,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[]
[null,"详情看文件夹","Hydraul_Test"]

{"sheet":"北醒测试","index":2,"n_rows":2,"n_cols":3,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
[]
[null,"详情看文件夹","Hydraul_Test"]

{"sheet":"放大晶体管测试","index":3,"n_rows":7,"n_cols":3,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
[]
[]
[null,"测试方法："]
[null,null,"1）ACR带载放大板，放大板输出接电磁阀"]
[null,null,"2）软件输出吸合电磁阀10s，断开20s。"]
[null,null,"3）测量方法板工作的mos管的发热程度"]
[null,null,"4）记录10min，30min，1h，2h，3h，4h，5h，6h,7h,8h的mos管的温度"]

{"sheet":"光电测试","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}

{"sheet":"整车功耗测试原始资料图","index":5,"n_rows":416,"n_cols":7,"rows_kept":416,"cut":false,"hidden":false,"merged":[]}
[]
[null,"测试目的：","了解整车各个环节的瞬时功率，确定电池与电源模块的选型合理性。完善设计文档。估算运行时长与充电时长"]
[]
[null,"测试说明：","测量各个分支的电流与电压，确定额定功率与最大功率值"]
[]
[]
[]
[null,"电气图"]
{"$rows_empty":21}
[null,"状态","电压（mV）","电流(mA)","功耗（W）","容量","温度"]
[null,"停止空载",52970,730,null,87,6]
[null,"停止空载",52970,680,null,87,6]
[null,"停止空载",52970,770,null,87,6]
[null,"停止空载",52970,680,null,87,6]
[null,"停止空载",52970,770,null,87,6]
[null,"行走空载",52970,3300]
[null,"行走空载",52970,3070]
[null,"行走空载",52970,3300]
[null,"行走空载",52970,3440]
[null,"行走空载",52970,3210]
[null,"满转空载",52970,5470]
[null,"满转空载",52970,5550]
[null,"满转空载",52970,5880]
[null,"满转空载",52970,5470]
[null,"满转空载",52970,5550]
[]
[null,"停止满载",52970,730,null,87,6]
[null,"停止满载",52970,680,null,87,6]
[null,"停止满载",52970,730,null,87,6]
[null,"停止满载",52970,680,null,87,6]
[null,"停止满载",52970,680,null,87,6]
[null,"行走满载",52970,3810,null,87,6]
[null,"行走满载",52970,4080,null,87,6]
[null,"行走满载",52970,3940,null,87,6]
[null,"行走满载",52970,3440,null,87,6]
[null,"行走满载",52970,4080,null,87,6]
[null,"满转满载",52970,17050,null,87,6]
[null,"满转满载",52970,10980,null,87,6]
[null,"满转满载",52970,11350,null,87,6]
[null,"满转满载",52970,11390,null,87,6]
[null,"满转满载",52970,11390,null,87,6]
[null,"换向满载",52970,21510,null,87,6]
[null,"换向满载",52970,16320,null,87,6]
[null,null,52970,21460,null,87,6]
{"$rows_empty":51}
[null,null,null,"停止空载"]
{"$rows_empty":47}
[null,null,null,"满转空载"]
{"$rows_empty":48}
[null,null,null,"顶升 空"]
{"$rows_empty":47}
[null,null,null,"满载停止"]
{"$rows_empty":32}
[null,null,null,"满载满转"]
{"$rows_empty":77}
[null,null,null,"换向满载"]
{"$rows_empty":43}
[null,null,null,"1500满转"]